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	Survey Checklist –Voyage Data Recorder (VDR) and Simplified Voyage Data Recorder (S-VDR)
Annual/Periodical/Renewal Surveys

	

	International Convention for the Safety of Life at Sea, 1974 as amended, Chapter V – Safety of Navigation

	This checklist is to be used for Annual/Periodical/Renewal Surveys. The annual performance test of VDR (or S-VDR) shall be carried out within the “time window” of the annual / periodical / renewal survey under the Harmonized System of Survey and Certification (HSSC), but not later than the date of completion of the survey for endorsement / renewal of the relevant Certificate.

	Survey requirements for passenger ships irrespective of size and cargo ships of 3000 gross tonnage and upwards

	
	Particulars of ship

	Name of ship
	     

	Flag
	     

	IMO number
	     

	Gross tonnage
	     

	Date on which keel was laid
	[bookmark: LR_O_KeelLaid]     

	Complete all relevant sections, providing information where required. 
Mark "Yes" to indicate complied with, "No" for not complied with and "NA" for not applicable. Where the response "No" is entered a remark is to be provided in paragraph CA.

	AA
	General

	
	Voyage data recorder details

	050
	Manufacturer
	     

	100
	Model
	     

	150
	System serial number
	     

	200
	Software version number
	     

	250
	Date fitted
	[bookmark: P1AA5]     

	

	BA
	Inspection Details

	050
	Name of person conducting testing
	     

	100
	Company
	     

	150
	Inspection Date
	     

	200
	Inspection location
	     

	

	BB
	Pre-existing alarms

	050
	Confirm that no alarms were present at start of survey
	

	

	BC
	Power supply alarm check

	050
	Remove source of external power. Confirm that alarm is activated.
	

	
	Record time (hh.mm) 
	[bookmark: P1BC2]  :  

	

	BD
	Reserve power source check

	
	Allow VDR to continue running for 1 hour 55 minutes from item BC050 above

	050
	Confirm that equipment is still operating at this time, with no additional alarms.
	

	
	Record time (hh.mm) 
	[bookmark: P1BD2]  :  

	

	BE
	Reserve power source shutdown check

	050
	2 hours 05 minutes from item BC050 above confirm that the VDR has automatically stopped recording.
	

	
	Record time (hh.mm) 
	[bookmark: P1BE2]  :  

	BF
	Battery expiry dates 

	
	Battery 
	Expiry Date (where applicable)

	050
	Acoustic beacon
	[bookmark: P1BF2]     

	100
	Reserve power source
	[bookmark: P1BF3]     


 




* Delete as appropriate
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	BG
	Acoustic beacon test

	050
	Using manufacturer’s test equipment, or by the substitution of a certified fully operational unit, confirm that acoustic beacon is functional
	

	

	BH
	Overall condition of equipment

	
	Is equipment in satisfactory condition? (record condition)

	[footnoteRef:1]*150 [1: * Delete as appropriate
] 

	Equipment
	Notes on condition

	050
	Protective capsule and release mechanism
	     
	

	100
	External cables
	     
	

	150
	Main unit
	     
	

	200
	Protective capsule float free arrangements where fitted
	     
	[bookmark: P1BHDropdown4]

	

	BI
	Interfaces:  Operation and recording

	
	Are the following interfaces operating and recording satisfactorily?

	
	Information
	Source

	050
	Date and time
	Preferably external to ship (e.g. Global  Navigation Satellite System)
	

	100
	Ship’s position
	Electronic Positioning system
	

	150
	Speed (through water or over ground)
	Ship’s designated speed and distance measuring equipment
	

	200
	Heading
	Ship’s compass
	

	250
	Bridge audio
	A minimum of two channels of audio with bridge wing audio recorded separately
	

	300
	Communications Audio
	VHF
	

	350
	Radar data-post display selection
	

	
	VDR approved to resolution MSC.333(90) or MSC.333(90) as amended by MSC.494(104):
	Both radar displays
	

	
	VDR or S-VDR approved to Res A.861(20) or Res MSC.163(78)
	Master radar displays
	

	400
	Water depth
	Echo sounder
	

	450
	Main alarms
	All mandatory alarms on bridge, Resolution A.1021(26) Table 10.1.1
	

	500
	Rudder order and response
	Steering gear and autopilot
	

	550
	Engine order and response
	Telegraphs, controls and thrusters
	

	600
	Hull openings status
	All mandatory status  information displayed on bridge
	

	650
	Watertight and fire door status
	All mandatory status  information displayed on bridge
	

	700
	Acceleration and hull stresses
	Hull stress and response monitoring equipment - where fitted
	

	750
	Wind speed and direction
	Anemometer - where fitted
	

	800
	Bridge watch alarm
	BNWAS 
	[bookmark: P2BIDropdown16]

	
	And for equipment approved to Res MSC.333(90):

	850
	Electronic Chart, Display and Information System
	ECDIS - where fitted
	[bookmark: DD02]

	900
	Automatic Information System
	All AIS Data
	[bookmark: dd03]

	950
	Rolling Motion
	Electronic inclinometer - where fitted
	

	1000
	Configuration Data
	Data block defining configuration of VDR and its sensors
	[bookmark: dd04]

	1050
	Electronic Logbook
	Where fitted
	[bookmark: dd05]

	

	BJ
	Completion of tests

	050
	Confirm that the recorder is restored to the normal operating mode following completion of the tests
	

	

	BK
	Change or repair of sensors

	050
	Are VDR maintenance records being maintained satisfactorily?
	

	100
	Are defects properly rectified?
	

	150
	Person authorised by the Manufacturer
	Ship’s representative

	
	Date
	Date

	
	     
	     

	

	BL
	Float-free capsule

	050
	For float-free capsules approved in accordance with resolution MSC.333(90) or MSC.333(90) as amended by MSC.494(104):
Ship’s representative
	

	
	Has an examination according to MSC.1/Circ.1040/Rev.2 been conducted?
	[bookmark: dasdad]

	










	BM
	Manufacturer’s analysis

	
	If the manufacturer does not complete a review and issue an Annual Performance Test Certificate within 45 days, this test report should be considered for Cargo Ship Safety Equipment or Passenger Ship Safety Survey certification.

	
	Note – This confirms the endorsement by the manufacturer of the tests and that the master record/database has been checked.
	

	050
	Is the manufacturer’s analysis of the 12-hour log attached?
	[bookmark: P2BKDropdown1]

	100
	Is the 12-hour log in accordance with International Electrotechnical Commission (IEC) 61996 Maritime navigation and radiocommunication equipment and systems – Shipborne voyage data recorder (VDR) – Performance requirements – Methods of testing and required test results section 4.6 – Data items to be recorded (resolution A.861(20), section 5.4).  
	

	150
	Is all the data from throughout the 12-hour recording available?
	

	200
	Date of log
	     
	Time of log
	     









	BN
	Observations and additional manufacturer’s requirements

	050
	Detail any significant events (including refitting of equipment or major unit change) that have occurred since the previous test
	

	
	[bookmark: Text1]     
	

	100
	Confirm that these events do not impact on the availability or quality of the VDR/S-VDR input signals
	

	

	CA
	Remarks

	
	     
	

	

	This performance test was conducted in accordance with SOLAS regulation V/18.8 and forms part of the procedure for the issue of the Annual Performance Test Certificate.  The results, information and any comments should be relayed to the manufacturer in accordance with the instructions contained within the Operation Manual.  Subject to satisfactory results, an Annual Performance Test Certificate will then be issued.

	In accordance with the principles of harmonization of Certificates, the Certificate, when issued, will remain valid until the next annual re-validation of that Certificate, subject to the equipment being maintained in appropriate operational condition.

	

	For completion and signature when the manufacturer has not elected to apply MSC.1/Circ.1222/Rev.1  in entirety

	[bookmark: P2Dropdown]This is to certify that an  survey of the Voyage Data Recorder has been carried out in accordance with the relevant regulations of the Convention and as described above:

	

	Inspected by

	Name of person conducting testing
	     
	Signature

	Inspection Company
	     
	

	Inspection Location
	     
	

	Inspection Date
	     
	

	

	Accepted by

	Surveyor
	     
	Signature

	Port
	Yokohama, Kobe or Nagasaki
	

	Date
	     
	[bookmark: LR_O_Represents]Surveyor to Lloyd's Register Group Limited
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	a member of the Lloyd's Register group.
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